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#241CN Homag BOF 32/50/G CNC Machining Center:
HOMAG BOF 32/50/G, YEAR  1999, 2-HEAD CNC ROUTER, HOMAG PROCESSING CENTER WITH TRIMMING, PROFILING, SHAPING, & BORING OF SOLID WOOD, MAN-MADE SHEET STOCK, OR COMPOSITE MATERIAL. • EQUIPPED AS FOLLOWS; WORKTABLE FOR MAX. WORKPIECE LENGTH OF 7,950 MM (316.229"), MAX. WORKPIECE WIDTH OF 1,370 MM (53.937") & MAX. WORKPIECE THICKNESS OF 70 MM (2.755"). • (2) MAIN WORK SPINDLES, EACH WITH A 12 KW (16 HP) WATER COOLED ROUTER WITH HSK F63 - DIN 69893 TOOL HOLDING SYSTEM FOR 1,500 - 18,000 RPM. THE ROUTER HAS C-AXIS TO ALLOW TOOL ROTATION OF 0° - 360° OF AGGREGATES FOR SAWING, TRIMMING, DRILLING, ETC.; ROUTER SPINDLE USES ATC PLATE-TYPE TOOL CHANGER WITH 18-TOOL POSITIONS FOR EACH ROUTER HEAD. • THE FOLLOWING TOOLS CAN BE USED: (18) TOOLS W/MAX. DIA. OF 120 MM (4.724") OR (9) TOOLS W/MAX. DIA. OF 160 MM (6.299"); (9) TOOLS W/MAX. DIA. OF 50 MM (1.968"). • INCLUDES: (2) DRILLING HEADS WITH (29) SPINDLES, (12) SPINDLES IN THE  X-AXIS & (19) SPINDLES IN THE Y-AXIS; ALL SPINDLES ARE ON 32 MM CENTER DISTANCE. • ADDITIONALLY INCLUDES: (6) SPINDLES FOR HORIZONTAL DRILL, (4) SPINDLES IN THE X-AXIS FOR DRILLING ON THE L & R PANEL EDGES & (2) SPINDLES IN THE Y-AXIS FOR DRILLING ON THE FRONT & BACK PANEL EDGES. • WORKTABLE: HIGH DENSITY LAMINATED WOODED PANEL FOR THE MOUNTING OF VACUUM CUPS FOR WORKPIECE CLAMPING; CLAMPING TABLE INTEGRATED IN THE MACHINE BED W/(12) SUBMERGING LONG STOPS 140 MM (5.512") & (2) SUBMERGING SIDE

STOPS. THE MACHINE ZERO-POINT IS PLACED AT THE LEFT FRONT SIDE & THE WORKPIECES ARE PLACED MANUALLY ON THE WORKTABLE. • HOMATIC CONTROL SYSTEM WITH: SPS CONTROL, 14" VGA COLOR MONITOR & 170 MB HARD DISK, 3D-LINEAR INTERPOLATION, 2 1/2 D-CIRCULAR INTERPOLATION, & 4-AXIS CONTROL (X, Y, Z, C). C-AXIS IS COUPLED TO THE X- & Y-AXIS, WOODWOP PROGAMMING SYSTEM, POST PROCESSOR CREATES CNC PROGRAMS IN DIN 66025 IN CONNECTION WITH WOODWOP & NETWORK CONNECTION FOR ARCNET OR ETHERNET W/TCP/IP & AUI CONNECTION. (2) VACUUM PUMPS RATED AT 100 CBM/HR FOR CLAMPING SYSTEM, LASER FOR POSITIONING OF THE VACUUM CUPS, LARGE QUANTITY OF AGGREGATE TOOLING. 
Selling Price: $49,999.
USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY.

