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#353CN – Friulmac Randomat E End Profiler:
	

	

	Friulmac end profiler, model Randomat E, demo model, year of mfg 2004, end profiling machine for random length material, set up to profile both ends of cabinet door rails, without changeover for various lengths, requires precision length precutting of incoming parts, parts are fed end to end with spacing allowing mixed sizes of doors to be processed together, perfect for building to order, each motor is adjustable separately, feed motor in/out 0.5 kW each, positioning motor 0.75 kW each, spindle diameter 40 mm, tool cutting circles 160 mm - 220 mm, motor capacity 5.5 kW (7.5 HP), out feed table length 3000 mm, in feed table length 3000 mm, production capacity up to 12 pcs/min, length of work piece min. 7" and max. 79" (180 mm - 2000 mm), width of work piece min. 1 3/16" and max. 9 3/16" (30 mm -250 mm), thickness of work piece min. 3/8" and max. 1 3/16" (10 mm - 30 mm), CSA approved components with Ontario Hydro approval
Selling Price $



USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY. SPECIFICATIONS ARE NOT ALWAYS EXACT AND ARE SUBJECT TO VERIFICATION.
