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#140CN – Selco EB120 Automatic Panel Saw:

Front load automatic panel saw, 176" overall cutting length (4,400mm), 4.7" (120mm) max. saw blade projection, 18kW (24HP) motor and 2.6kW (3.5HP) scoring motor, modular roller rear machine table, side aligning device and 2 logitudinal aligners to accurately position book of panels on rear saw table prior to cutting, variable saw carriage travel speed from 0 -328FPM, obtained by a brushless Servomotor with digital technology ensures a real CNC control without the use of sensors or microswitches, electronically controlled overhead program fence, rack and pinion driven, forward speed of 196FPM, return speed of 196FPM, main saw blade projection is automatically adjusted according to the stack height selected, ensuring optimum cutting quality, equipped with: (7) self-leveling grippers (open up to 122mm), of which (3) are closely spaced in crosscut area and the other (4) are at equal distance in rip cut area, design of structure and machine logic allow the total ejection of the cut stack of panels beyond the cutting line which facilitates the removal of the trim cuts produced, AC brushless servomotor with digital technology under direct monitoring of numerical control drives the pusher fence, NC 410 control with color monitor inegrated into high-tech look operator control panel (displays cutting dimensions and patterns), (100) cutting patterns with (50) different dimensions for each pattern, self-diagnostic, data input by keyboard or possible direct downloading from office PC, machine equipped with 2,300mm long crosscut fence stroke (side to side), (2) side/crosscut aligners , (3) front mounted air float tables with rounded front for moving panel from rip to crosscut position (24" x 79" each), rear of machine partially enclosed for safety, year 2001
Selling Price: $44,000.

USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY.
