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#186CN – Midwest Countertop Station:
Counter top saw for cutting off or mitering postformed, self-edged, coved or solid surface countertops and draw-bolt mortising in one single operation, 5HP belt driven main motor, 0.5HP feed drive motor, variable feed speed from 0 - 45 FPM, 45 FPM fixed return speed, 16" diameter blade, 1" diameter arbor, 3,400 RPM blade speed, 5-5/8" depth of cut with build-down, 4-7/8" without build-up, 3/4" max. build-up thickness, 4-7/8" max back splash height, 42" crosscut capacity at 90 degrees, 38" at 22-1/2 degrees, 30" cut at 45 degrees, upper machine structure rotates left and right to 5 fixed stops at miter positions: 90, 45R&L, 22-1/2R&L degrees, new routers for routing the draw bolt mortises, pneumatic holddowns.
Selling Price: $15,000.

USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY.
