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# 113CN – Norfield 3800 Door Machine (USED):
Door router for lock and latch, routing and face plating of any length wood or metal door slab, maximum door width 4`, lockbore sizes 1-1/2" - 2-1/8", door thickness 1-3/4", lock backset 2-3/8" - 2-3/4", faceplate width adjustable to 1-1/8", faceplate length adjustable to 2-1/2", templates must be at least 80" tall and 9" wide so that there are a total of four lamps in contact, the O/H system can house any style and you can switch between a 22*36 to a 22*64 by raising the drop bar, tool offset 1/2"/side - template opening is 1" larger than cutout, the 4 hole rotary lock template can be used for 2-1/8", 1-7/8", 1-5/8" & 1-1/2".
Selling Price $16,000.
Used machinery is sold “as is” and is not covered under warranty

