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#320CN – Ligmatech Return Conveyor:
Automatic boomerang return conveyor for edgebander, model ZHR15, for edgebander left hand machine, transfers panels to conveyor for return to operator, once edgebanded the panels are lifted upwards by a unique scissor action and transferred to a top feeder unit, the unit feeds the panels onto a gravity roller track for return to operator, unit also incorporates a rotary transfer device, when a panel is fed cross-wise through the edgebander the rotary transfer device will rotate them length wise for return on the gravity roller track, working length max. 2500mm min. 300mm, working width max. 1000mm min. 120mm, working thickness max. 50mm, panel weight 50kgs max., 30kgs with turning, working speed max. 48 m/min, min. 8m/min, electrical consumption 1.0kW, operating pressure 6 bar, air 90psi, length of edgbanding m/c 8500mm (28'), replacement cost approx. $40,000
Selling Price: $15,000.
USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY.
